#
# Sample boot menu configuration file
#

# Boot automatically after 30 secs.
timeout 30

# By default, boot the first entry.
default 0

# Fallback to the second entry.
fallback 1

# For booting GNU/Hurd
title  GNU/Hurd
root   (hd0,0)
kernel /boot/gnumach.gz root=hd0s1
module /boot/serverboot.gz

# For booting GNU/Linux
title  GNU/Linux
root (hd1,0)
kernel /vmlinuz root=/dev/hdb1
#initrd /initrd.img

# For booting GNU/kFreeBSD
title  GNU/kFreeBSD
root   (hd0,2,a)
kernel /boot/loader.gz

# For booting GNU/kNetBSD
title  GNU/kNetBSD
root   (hd0,2,a)
kernel --type=netbsd /boot/knetbsd.gz

# For booting Mach (getting kernel from floppy)
title  Utah Mach4 multiboot
root   (hd0,2)
pause  Insert the diskette now!!
kernel (fd0)/boot/kernel root=hd0s3
module (fd0)/boot/bootstrap

# For booting FreeBSD
title  FreeBSD
root   (hd0,2,a)
kernel /boot/loader

# For booting NetBSD
title  NetBSD
root   (hd0,2,a)
kernel --type=netbsd /netbsd

# For booting OpenBSD
title  OpenBSD
root   (hd0,2,a)
kernel --type=netbsd /bsd

# For booting OS/2
title OS/2
root  (hd0,1)
makeactive
# chainload OS/2 bootloader from the first sector
chainloader +1
# This is similar to "chainload", but loads a specific file
#chainloader /boot/chain.os2

# For booting Windows NT or Windows95
title Windows NT / Windows 95 boot menu
rootnoverify (hd0,0)
makeactive
chainloader  +1
# For loading DOS if Windows NT is installed
# chainload /bootsect.dos

# For installing GRUB into the hard disk
title Install GRUB into the hard disk
root    (hd0,0)
setup   (hd0)

# Change the colors.
title Change the colors
color light-green/brown blink-red/blue
