REGISTER WINDOW

The quick help bar shows most of the available keypresses across the bottom of the screen. Use the cursor keys to move around the display and the 0 to 9 and A to F keys to change the hexadecimal register values.

The following chart shows the keypress and functions for the Register window.

Keypress | Function
F3-Expr | Allows entry of an expression to set the register value.
Alt-F3-List | Displays a list of symbols. Highlight the symbol you want to move the display to and press enter. Symbols are listed with names on the left and values on the right. The C or D displayed adjacent to the value indicates the address type is CODE or DATA. A speed search is available by typing the desired symbol text. Backspacing to eliminate mistyped characters is supported. Using this function on EIP sets CS and moves the CS:EIP window to the chosen address.
F5-FPU | Show floating point registers in FPU if present.
+ | Increments the current register value.
- | Decrements the current register value.
Alt-X | Exit to DOS.

Next Page

Previous Page

Go to Table of Contents