Next, protected mode interrupt vectors are listed with the following headings:

No sel offset

Where:

No

Vector number.

sel

Selector value for handler.

offset

Offset value for handler.

This information allows a cross-reference with the other lists to ensure CauseWay application installed handlers have been properly made.

Next, protected mode exception vectors are listed using the same format as protected mode interrupts.

After the protected mode exception vector list, real mode interrupt vectors are listed. They are shown in the same format as protected mode interrupts although the selector values are real mode segment values.

Only those interrupt and exception vectors altered by the program will be listed.

Lastly, Call-Backs are listed in the CW.ERR file. They list all active Call-Backs for the active application at the time of its termination.

Next Page

Previous Page

Go to Table of Contents